Fecha/hora: 03/06/2024 05:43:08

Biblioteca(s): 	INIA La Estanzuela.	
Tipo de la producción científica: 	Artículos en Revistas Indexadas Internacionales	
Circulación/Nivel: 	Internacional - --	
Fecha corriente: 	16/12/2021	
Fecha de la última actualización: 	02/09/2022	
Autoria: 	RACHID, C.; RESQUÍN, F.; CARRASCO-LETELIER, L.	
Afiliación: 	ANA CECILIA RACHID CASNATI, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; JOSE FERNANDO RESQUIN PEREZ, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; LEONIDAS CARRASCO-LETELIER, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay.	
Título: 	Availability and environmental performance of wood for a second-generation biorefinery.	
Año de publicación: 	2021	
Fuente/Imprenta: 	Forests 2021, Volume 12, Issue 11, Article 1609; Open Access. Doi:https://doi.org/10.3390/f12111609	
DOI: 	10.3390/f12111609	
Idioma: 	Inglés	
Notas: 	Article history: Received: 5 October 2021 / Revised: 28 October 2021 / Accepted: 29 October 2021 / Published: 22 November 2021.	
Contenido: 	Abstract:
The current global climate change, the 2030 Agenda, and the planetary boundaries have driven new development strategies, such as the circular economy, bioeconomy, and biorefineries. In this framework, this study analyzes the potential availability and sustainability of the wood supply chain for a small-scale biorefinery aiming at producing 280?300 L of bioethanol per ton of dry biomass, consuming 30,000 t of dry biomass per year harvested in a 50 km radius. This wood production goal was assessed from Eucalyptus grandis stands planted for solid wood in northeastern Uruguay. Moreover, to understand the environmental performance of this biomass supply chain, the energy return on investment (EROI), carbon footprint (CF), and potential soil erosion were also assessed. The results showed that the potential wood production would supply an average of 81,800 t of dry mass per year, maintaining the soil erosion below the upper threshold recommended, an EROI of 2.3, and annual CF of 1.22 kg CO2?eq m?3 (2.6 g CO2?eq MJ?1). Combined with the environmental performance of the bioethanol biorefinery facility, these results would show acceptable values of sustainability according to EU Directive 2009/28/ec because the bioethanol CF becomes 1.7% of this petrol?s CF	
Palabras-Clave: 	Bioethanol; Carbon footprint; EROI; Eucalyptus; SOIL EROSION.	
Categoría del tema: 	--	
URL: 	http://www.ainfo.inia.uy/digital/bitstream/item/16679/1/forests-12-01609-v3.pdf
https://www.mdpi.com/1999-4907/12/11/1609	
Registro original: 	INIA La Estanzuela (LE)	
Ejemplares: 	LE - (103473-1) - PXI - AP - DD - PP/Forests 2021 -  -  - DIS