Fecha/hora: 16/06/2024 11:27:22

Biblioteca(s): 	INIA La Estanzuela; INIA Tacuarembó.	
Fecha corriente: 	10/08/2016	
Fecha de la última actualización: 	05/11/2019	
Autoria: 	LOPRETTI, M.I.; BALDYGA, N.T.; GONZALEZ, M.; OLAZABAL, L.B.; TORRES,  M.G.; RESQUÍN, F.; CARRASCO-LETELIER, L.	
Afiliación: 	JOSE FERNANDO RESQUIN PEREZ, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; LEONIDAS CARRASCO-LETELIER, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay.	
Título: 	Biodegradation pretreatment of wood of E. grandis, E. dunnii, and E. benthamii to work in biorefinery processes.	
Año de publicación: 	2016	
Fuente/Imprenta: 	Journal of Renewable Materials, v. 4, n. 1, p. 66-71, 2016.	
DOI: 	10.7569/JRM.2015.634133	
Idioma: 	Inglés	
Notas: 	Article history: Received October 13, 2015/ Accepted January 21, 2016.	
Contenido: 	Nowadays, there is a great interest in using lignocellulosic materials as substrate for the production of
biorefi nery products. Eucalypti are good options to use as crops to obtain different kinds of biofuels and
derivatives, since their plantations show high adaptation potential to soil and weather conditions in Uruguay.
The basic process steps involved in the obtainment of biorefi nery materials are: pretreatment, hydrolysis,
fermentation and products separation. As delignifi cation is an important process to obtain biorefi nery products,
in this context the evaluation of the biological (BT) and hydrothermal (TT) pretreatment of different species of
Eucaliptus was studied. The possibility of obtaining sugars, alcohols and organic acids was the main focus.
The results of these investigations show a good production of reducing sugars (4?5 mg/mL for both BT and
TT pretreatments), acetic acid (3?8 mg/mL for BT and 3?7 mg/mL for TT) and isopropanol (18?48 mg/mL for
BT and 20?30 mg/mL for TT). In conclusion, the results show similar behaviours for BT and TT pretreatments,
which is a quite important result since BT is cheaper and cleaner and thus a more attractive technology.	
Palabras-Clave: 	BIOREFINERY; BIORREFINERÍA; DELIGNIFICATION; PRETRATAMIENTO; PRETREATMENT.	
Thesagro: 	BIODEGRADACION; MADERA.	
Categoría del tema: 	K10 Producción forestal	
Registro original: 	INIA La Estanzuela (LE)	
Ejemplares: 	LE - (101467-1) - PXI - AP - DD - PP/J. Renew. Mater/2016 -  -  - DIS
TBO - (101349-1) - PXI - AP - DD - PP/JOURNAL OF RENEWABLE MATERIALS/1/2016 -  -  - DIS