Fecha/hora: 03/06/2024 05:05:29

Biblioteca(s): 	INIA Las Brujas.	
Tipo de la producción científica: 	Artículos en Revistas Indexadas Internacionales	
Circulación/Nivel: 	B - 2	
Fecha corriente: 	29/05/2017	
Fecha de la última actualización: 	29/05/2017	
Autoria: 	PUPPO, L.; GARCIA, C.; GIRONA, J.; GARCÍA-PETILLO, M.	
Afiliación: 	L. PUPPO, Grupo Disciplinario de Ingeniería Agrícola, Unidad de Hidrología, Departamento de Suelos y Aguas-Facultad de Agronomía, Universidad de la República, Montevideo, Uruguay; CLAUDIO CESAR GARCIA GALLARRETA, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; J. GIRONA, Institut de Recerca i Tecnologia Agroalimentàries (IRTA), Programa Uso Eficiente del Agua, Centre UdL-IRTA Parc de Gardeny, Edifici Fruitcentre, Lleida, Catalunya, España; MARIO GARCÍA-PETILLO, Grupo Disciplinario de Ingeniería Agrícola, Unidad de Hidrología, Departamento de Suelos y Aguas-Facultad de Agronomía, Universidad de la República, Montevideo, Uruguay.	
Título: 	Determination of young olive-tree water consumption with drainage lysimeters.	
Año de publicación: 	2014	
Fuente/Imprenta: 	Journal of Water Resource and Protection, 2014, v. 6, pp. 841-851.	
DOI: 	10.4236/jwarp.2014.69079	
Idioma: 	Inglés	
Notas: 	This article belongs to the Special Issue on Evapotranspiration.
Article history: Received 1 March 2014; revised 28 March 2014; accepted 21 April 2014.	
Contenido: 	ABSTRACT.
Information about olive-tree irrigation in sub-humid climates, as in Uruguay, is scarce. Water consumption of young olive trees, Arbequina variety, was measured for two years with six drainage lysimeters, protected from rain by an automatic rain-out shelter. Irrigation water volume and drainage of each lysimeter were measured daily and soil moisture was registered twice a week with neutron probe at four depths. Evapotranspiration (ETc) was calculated by volume balance. Data periods when available water descended below 50% or increased over 100% were eliminated, as those in which the stem water potential was below ?1.5 MPa. Water consumption values were averaged within 7- to 14-day periods, expressed in mm·d?1, and referred to a 2.5 × 5.5 m plantation framework without vegetation cover. There was a positive linear relation of the summer crop coefficient (Kc mid) with age, canopy cover percentage and canopy volume. Canopy cover percentage was the parameter which explained most of the variation of Kc mid, which ranged between 0.13 and 0.24, with 5% and 46% canopy cover, respectively. Full irrigation, associated to a good drainage resulted in a rapid growth of the young plants, bringing forward the start  f full  production period. This represents useful information for the adjustment of irrigation in olive-tree orchards, to accelerate growth with a rational and sustainable use of both water and
energy in Uruguay.	
Palabras-Clave: 	CROP COEFFICIENTS; EVAPOTRANSPIRATION; IRRIGATION REQUIREMENTS.	
Thesagro: 	BALANCE HIDRICO; EVAPOTRANSPIRACION; OLEA EUROPAEA L.	
Categoría del tema: 	--	
URL: 	http://file.scirp.org/pdf/JWARP_2014062616310711.pdf	
Registro original: 	INIA Las Brujas (LB)	
Ejemplares: 	LB - (101401-1) - PXI - AP - DD - PP/JWARP/2014 -  -  - DIS