Fecha/hora: 11/05/2024 17:41:42

Biblioteca(s): 	INIA La Estanzuela; INIA Las Brujas.	
Fecha corriente: 	21/02/2014	
Fecha de la última actualización: 	10/05/2018	
Autoria: 	GARCIA, C.; CARLESSO, R.; ROSA, G.M.; PETRY, M.T.; MELO, G.L.	
Afiliación: 	CLAUDIO CESAR GARCIA GALLARRETA, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; R. CARLESSO; G.M. ROSA; M.T. PETRY; G.L. MELO.	
Título: 	Water deficit effects on maize yield in southern Brazil.	
Año de publicación: 	2002	
Fuente/Imprenta: 	ln: Workshop em Engenharia Agrícola (2002 : Santa Maria, RS), Mostra dos trabalhos científicos do PPGEA do ano de 2002 / Santa Maria, RS : Universidade Federal de Santa Maria, Centro de Ciências Rurais, Programa de Pós-Graduação em Engenh 2002.	
Páginas: 	p. 224-228	
Idioma: 	Inglés	
Notas: 	Trabajo presentado en la ASAE Annual International Meeting 2002 / CIGR XV World Congress Sponsored by ASAE and  CIGR, Hyatt Regency Chicago, Chicago, Illinnois, USA July 28-July 31, 2002 Brasil. Ministério da Educaçao; Universidade Federal de Santa María. Centro de Ciencias Rurais. Programa de Pós-Graduaçao em Engenharia Agrícola	
Contenido: 	ABSTRACT: 
The objective of this experiment was to evaluate the water deficit effects on maize yield and yield components. The maize hybrid Pioneer 30F33 was submitted to five irrigation water management treatments. Irrigation management was based on crop maximum evapotranspiration (ETm). Irrigations were applied when cumulative ETm reached values of 14, 22, 30, 38 and 46 mm. The experiment was conducted on a set of 20 drainage lysimeters under a mobile rain shelter. Leaf area index and plant height were measured twice a weak in each
treatment from 29 days after emergency to harvest. Soil moisture were measure in each soil !ayer (0-20; 20-40; 40-53; 53-66 and 66-100 cm), twice a weak. Results of leaf area and plant height were similar during crop growing season for ali irrigation strátegies, and aboveground biomass accumulation at harvest was also similar for ali treatments. Maximum technical maize yield was obtained applying irrigation when cumulative ETm reached value of the 34 mm. Total irrigation depth applied was 264, 281, 278, 279, and 282 mm using the irrigation
management of 14, 22, 30, 38 e 46 mm of cumulative ETm. The use of irrigation application based on cumulative ETm values in Southern Brazil results in a easier practice to increase water use efficiency, increase maize yield and reduce application cost.	
Palabras-Clave: 	EVAPOTRANSPIRATION; IRRIGATION MANAGEMENT; MAIZE.	
Thesagro: 	EVAPOTRANSPIRACION; MAIZ; MANEJO DEL SUELO; RIEGO.	
Categoría del tema: 	--
P10 Recursos hídricos y su ordenación	
URL: 	http://www.ainfo.inia.uy/digital/bitstream/item/9533/1/Garcia-C.-2002.-PPGEA-2002-p.224-228.pdf	
Registro original: 	INIA Las Brujas (LB)	
Ejemplares: 	LB - (10843-1) - PXI - PL - PP - 631.587 - UFSMm 2002 - 2989 - DIS