Fecha/hora: 26/07/2024 21:33:02

Biblioteca(s): 	INIA La Estanzuela.	
Fecha corriente: 	09/10/2015	
Fecha de la última actualización: 	01/09/2022	
Autoria: 	BERGER, A.; OTERO, A.; MORALES, X.; CALISTRO, R.	
Afiliación: 	ANDRES GUSTAVO BERGER RICCA, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; ALVARO RICARDO OTERO CAMA, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; MARIA XIMENA MORALES LORENZONI, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; RICARDO ARIEL CALISTRO DIAZ, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay.	
Título: 	Actual evapotranspiration measurement trough [i.e. through] eddy covariance in Uruguay: abstract.	
Año de publicación: 	2015	
Fuente/Imprenta: 	Agrociencia Uruguay, v. 19, special issue "Inter-Regional CIGR Conference on Land and Water Challenges, 3., La Estanzuela, Colonia, UY. Tools for developing; "Dr. Mario García Petillo"", p. 4, 2015.	
ISSN: 	1510-0839.	
Idioma: 	Inglés	
Contenido: 	Tough there have been great advances in estimating actual evapotranspiration, achieving accurate estimates at the field level
is still a challenge. The characterization of site specific characteristics influencing evapotranspiration like soil properties impose
a great challenge to the use of modeling, and the accurate characterization of the variability within a field of crop status may bias
estimates. Using remote sensing to estimate crop status and energy balance at a fine scale overcome some of these issues.
Nevertheless there is a need to have accurate and precise measurements of evapotranspiration that can serve as validation
sites. The eddy covariance method provides the accuracy and footprint necessary to be used as a reference. Two towers were
installed between 2010 and 2015 at two contrasting locations each year in the south-west of Uruguay at agricultural fields with
wheat-soybean crop rotation. The sites were maintained at the same location during wheat and soybean, and were moved
when other crops were planted at the site. Each tower had instruments to measure in parallel the energy balance (radiometers,
flux plates and soil temperature probes), and evapotranspiration directly from eddy covariance (sonic anemometer, IRGA). All
locations met fetch requirements, were representative of agricultural fields and were situated in an area dominated by agricultural
land. Season long totals showed large variability depending on crop status and seasonal precipitation regime that determined
crop growth and leaf area development. Even after full canopy cover was reached (maximum Kc) there was large variation in
evapotranspiration reflecting periods of severe stress in some years. This study provides reference values for a significant
number of growing conditions and years and highlights the need for considering the variability among years and crops when
making estimates of demand for supplemental irrigation. It also provides reference values for methods based on remote
sensing of evapotranspiration.	
Palabras-Clave: 	ANÁLISIS DE COVARIANZA; COVARIANZA DE TORBELLINOS; ETA; EVAPOTRANSPIRACIÓN ACTUAL; FISIOLOGÍA VEGETAL; MEDICIÓN DE LA EVAPOTRANSPIRACIÓN; MEDIDA DE LA EVAPOTRANSPIRACIÓN.	
Thesagro: 	SOJA.	
Categoría del tema: 	F60 Fisiología y bioquímica de la planta	
URL: 	http://www.ainfo.inia.uy/digital/bitstream/item/5045/1/Agrociencia-Congreso-CIGR2015-v.19.si.p.4-BERGER.pdf	
Registro original: 	INIA La Estanzuela (LE)	
Ejemplares: 	LE - (101163-1) - INI - PC - PP - LE-PP/AGROCIENCIA URUGUAY/ - 2015/19/si - .. - DIS
LE - (101163-2) - INI - PC - DD -  -  -  - DIS