Fecha/hora: 20/05/2024 14:42:17

Biblioteca(s): 	INIA La Estanzuela; INIA Las Brujas.	
Fecha corriente: 	05/10/2015	
Fecha de la última actualización: 	15/03/2021	
Autoria: 	OTERO, A.; BERGER, A.; MORALES, X.; CALISTRO, R.	
Afiliación: 	ALVARO RICARDO OTERO CAMA, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; ANDRES GUSTAVO BERGER RICCA, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; MARIA XIMENA MORALES LORENZONI, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; RICARDO ARIEL CALISTRO DIAZ, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay.	
Título: 	Eddy covariance estimates of evapotranspiration in irrigated and rainfed soybean in Uruguay: abstract.	
Año de publicación: 	2015	
Fuente/Imprenta: 	Agrociencia Uruguay, 2015, v.19, Special Issue, Congreso CIGR. 3r. Inter-Regional CIGR Conference on Land and Water Challenges: Tools for developing "Dr. Mario García Petillo", p.8	
ISSN: 	1510-0839	
Idioma: 	Inglés	
Notas: 	EDITORIAL BOARD SPECIAL ISSUE: García, C. (Instituto Nacional de Investigación Agropecuaria); Puppo, L. (Universidad de la República, Facultad de Agronomía); Tarjuelo, J.M. (Univ. Castilla-La Mancha, España); Carsjens, G-.J. (Univ.Wageningen, Holanda).	
Contenido: 	Estimating total crop water use and the associated variability are critical for planning, for the design of supplementary irrigation
strategies and for subsequent management. Tough there have been great advances in estimating actual evapotranspiration,
achieving accurate estimates at the field level is still a challenge. The characterization of site specific characteristics influencing
evapotranspiration like soil properties impose a great challenge to the use of modeling, and the accurate characterization of the
variability within a field of crop status may bias estimates. Using remote sensing to estimate crop status and energy balance at
a fine scale overcome some of these issues. Nevertheless there is a need to have accurate and precise measurements of
evapotranspiration that can serve as validation sites. The eddy covariance method provides the accuracy and footprint
necessary to be used as a reference. Two towers were installed between 2010 and 2015 at two contrasting locations each year
in the south-west of Uruguay at agricultural fields with wheat-soybean crop rotation. The sites were maintained at the same
location during wheat and soybean. Sites were managed with supplementary irrigation at full demand or without irrigation. Each
tower had instruments to measure in parallel the energy balance (radiometers, flux plates and soil temperature probes), and
evapotranspiration directly from eddy covariance (sonic anemometer, IRGA). All locations met fetch requirements, were
representative of agricultural fields and were situated in an area dominated by agricultural land. Season long totals showed large
variability depending on crop status and seasonal precipitation regime that determined crop growth and leaf area development.
Totals for irrigated fields in the north (Salto, 650-800mm) were higher than in the south (Colonia-Soriano, 600-750), and higher
than standard requirements for the region. This study provides reference values for a significant number of growing conditions
and years for irrigated or rain-fed soybean crops.	
Palabras-Clave: 	COVARIANZA DE TORBELLINOS; COVARIANZA EDDY; COVARIANZA TURBULENTA; CULTIVO DE SECANO; CULTIVO IRRIGADO; ETA; EVAPOTRANSPIRACIÓN ACTUAL; MEDICIÓN DE COVARIANZA; MEDIDA DE COVARIANZA.	
Thesagro: 	EDDY COVARIANCE; EFICACIA EN EL USO DEL AGUA; ETA; GLYCINE MAX; SOJA; SOYBEAN; WATER USE EFFICIENCY.	
Categoría del tema: 	F60 Fisiología y bioquímica de la planta
P30 Ciencia del suelo y manejo del suelo	
URL: 	http://www.ainfo.inia.uy/digital/bitstream/item/5046/1/Agrociencia-Congreso-CIGR2015-v.19.si.p.8-OTERO.pdf	
Registro original: 	INIA Las Brujas (LB)	
Ejemplares: 	LB - (100669-1) - PXI - PL - PP - PP/AGROCIENCIA/2015/19/Sp.Issue -  - Agr.v.19. - DIS
LE - (101166-1) - PXI - PC - PP - LE-PP/AGROCIENCIA URUGUAY/ - 2015/19/si - ... - DIS
LE - (101166-2) - PXI - PC - DD -  -  -  - DIS