Fecha/hora: 16/06/2024 15:37:27

Biblioteca(s): | INIA La Estanzuela.
Fecha corriente: | 21/02/2014
Fecha de la última actualización: | 08/10/2019
Autoria: | MORON, A.; COZZOLINO, D.
Afiliación: | DAVID ALEJANDRO MORON YACOEL, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay; DANIEL COZZOLINO GÓMEZ, INIA (Instituto Nacional de Investigación Agropecuaria), Uruguay.
Título: | Exploring the use of near infrared reflectance spectroscopy to study physical properties and microelements in soils.
Año de publicación: | 2003
Fuente/Imprenta: | Journal of Near Infrared Spectroscopy, 2003, Volume 11, Issue 2, Pages 145-154.
DOI: | 10.1255/jnirs.362
Idioma: | Inglés
Notas: | Article history:

Contenido:

Abstract.
Near infrared (NIR) reflectance spectroscopy was used to predict the content of silt, sand, clay, iron (Fe), copper (Cu), manganese (Mn) and zinc (Zn) in soil. A total of 332 samples from agricultural soils (0?15 cm depth) in Uruguay (South America) were used. The samples were scanned in a monochromator instrument (NIRSystems 6500, Silver Spring, MD, USA). Two mathematical treatments (first and second derivative) with SNVD (scatter normal variate and detrend) and without scatter correction were studied. Modified partial least squares (mPLS) was used to develop the calibration models. The coefficient of determination in calibration (R2cal) and the standard error in calibration (SEC) using the second derivative were 0.81 (SEC: 5.1), 0.83 (SEC: 5.3), 0.92 (SEC: 2.6) for percent sand, silt and clay, respectively. The R2cal and standard error of cross-validation (SECV) were for Cu 0.87 (SEC: 0.7), for Fe 0.92 (SEC: 21.7), for Mn 0.72 (SEC: 83.0) and for Zn 0.72 (SEC: 1.2) on mg kg?1 dry matter. It was concluded that NIR reflectance spectroscopy has a great potential as an analytical method for routine analysis of soil texture, Fe, Zn and Cu due the speed and low cost of analysis

Palabras-Clave: | CLAY; COPPER; MANGANESE; NEAR INFRARED (NIR) SPECTROSCOPY; SAND; SILT.
Thesagro: | MAGNESIO; NIRS; SOIL; SUELO; ZINC.
Categoría del tema: | P35 Fertilidad del suelo
Registro original: | INIA La Estanzuela (LE)
Ejemplares: | LE - (49363-1) - PXI - AP - DD - PP/J.Near Infrared Spectroscopy/2003 -  -  - DIS